Reference

Abbas, S., & Lecampion, B. (2013). Initiation and breakdown of an axisymmetric hydraulicfracture transverse to a horizontal wellbore. Paper presented at the ISRM International Conference for Effective and Sustainable Hydraulic Fracturing, Paper Number: ISRM-ICHF-2013-001

Ahmed, S., Salehi, S., & Ezeakacha, C. (2020). Review of gas migration and wellbore leakage in liner hanger dual barrier system: Challenges and implications for industry. Journal of Natural Gas Science and Engineering, 78, 103284.

Allahvirdizadeh, P. (2020). A review on geothermal wells: Well integrity issues. Journal of cleaner production, 275, 124009.

Banthia, N., & Mindess, S. (1989). Water permeability of cement paste. Cement and concrete research, 19(5), 727-736.

Bear, J., & Corapcioglu, M. (1981). A mathematical model for consolidation in a thermoelastic aquifer due to hot water injection or pumping. Water Resources Research, 17(3), 723-736.

Biot, M. A. (1977). Variational Lagrangian-thermodynamics of nonisothermal finite strain mechanics of porous solids and thermomolecular diffusion. International Journal of Solids and Structures, 13(6), 579-597.

Cai, W., Deng, J., Luo, M., Feng, Y., Li, J., & Liu, Q. (2022). Recent advances of cementing technologies for ultra-HTHP formations. International Journal of Oil, Gas and Coal Technology, 29(1), 27-51.

Carnahan, C. (1983). Thermodynamic coupling of heat and matter flows in near-field regions of nuclear waste repositories. MRS Online Proceedings Library (OPL), 26.

Chen, G., & Ewy, R. T. (2005). Thermoporoelastic effect on wellbore stability. SpE Journal, 10(02), 121-129.

Cheng, A. H.-D. (2016). Poroelasticity (Vol. 27): Springer.

DeBruijn, G., Skeates, C., Greenaway, R., Harrison, D., Parris, M., James, S., . . . Temple, L. (2008). High-pressure, high-temperature technologies. Oilfield Review, 20(3), 46-60.

Delaney, P. T. (1982). Rapid intrusion of magma into wet rock: Groundwater flow due to pore pressure increases. Journal of Geophysical Research: Solid Earth, 87(B9), 7739-7756.

Denbigh, K. (1949). Thermo-osmosis of gases through a membrane. Nature, 163(4132), 60-60.

Derski, W. (1979). Equations of linear thermoconsolidation. Archives of Mech., 31(3), 303-316.

Detournay, E., & Cheng, A.-D. (1988). Poroelastic response of a borehole in a non-hydrostatic stress field. Paper presented at the International Journal of Rock Mechanics and Mining Sciences & Geomechanics Abstracts.

Detournay, E., & Cheng, A. H.-D. (1993). Fundamentals of poroelasticity. In Analysis and design methods (pp. 113-171): Elsevier.

Drake, J. A., Bradford, A., & Marsalek, J. (2013). Review of environmental performance of permeable pavement systems: state of the knowledge. Water Quality Research Journal of Canada, 48(3), 203-222.

Eshraghi, D. (2013). P&A-status on regulations and technology, and identification of potential improvements. University of Stavanger, Norway,

Gao, J., Deng, J., Lan, K., Song, Z., Feng, Y., & Chang, L. (2017). A porothermoelastic solution for the inclined borehole in a transversely isotropic medium subjected to thermal osmosis and thermal filtration effects. Geothermics, 67, 114-134.

Ge, Z., Yao, X., Wang, X., Zhang, W., & Yang, T. (2018). Thermal performance and microstructure of oil well cement paste containing subsphaeroidal konilite flour in HTHP conditions. Construction and Building Materials, 172, 787-794.

Ghabezloo, S., & Sulem, J. (2010). Temperature induced pore fluid pressurization in geomaterials. arXiv preprint arXiv:1011.6501.

Ghassemi, A., & Diek, A. (2002). Porothermoelasticity for swelling shales. Journal of Petroleum Science and Engineering, 34(1-4), 123-135.

Ghassemi, A., Tao, Q., & Diek, A. (2009). Influence of coupled chemo-poro-thermoelastic processes on pore pressure and stress distributions around a wellbore in swelling shale. Journal of Petroleum Science and Engineering, 67(1-2), 57-64.

Gomar, M., Goodarznia, I., & Shadizadeh, S. R. (2014). Transient thermo-poroelastic finite element analysis of borehole breakouts. International Journal of Rock Mechanics and Mining Sciences, 71, 418-428.

Gonçalvès, J., & Trémosa, J. (2010). Estimating thermo-osmotic coefficients in clay-rocks: I. Theoretical insights. Journal of colloid and interface science, 342(1), 166-174.

Goto, S., & Roy, D. M. (1981). The effect of w/c ratio and curing temperature on the permeability of hardened cement paste. Cement and concrete research, 11(4), 575-579.

Gruber, S., & Plank, J. (2021). *Challenges in Cementing Deep Offshore Wells.* VSOE2021 2021. Lecture Notes in Civil Engineering, vol 208. Springer, Singapore. https://doi.org/10.1007/978-981-16-7735-9\_51

Hargis, C. W., Chen, I. A., Devenney, M., Fernandez, M. J., Gilliam, R. J., & Thatcher, R. P. (2021). Calcium Carbonate Cement: A Carbon Capture, Utilization, and Storage (CCUS) Technique. Materials, 14(11), 2709.

Katende, A., Lu, Y., Bunger, A., & Radonjic, M. (2020). Experimental quantification of the effect of oil based drilling fluid contamination on properties of wellbore cement. Journal of Natural Gas Science and Engineering, 79, 103328.

Khalifeh, M., & Saasen, A. (2020). Introduction to permanent plug and abandonment of wells: Springer Nature.

Khalili, N., Geiser, F., & Blight, G. (2004). Effective stress in unsaturated soils: Review with new evidence. International journal of Geomechanics, 4(2), 115-126.

Kiran, R., Teodoriu, C., Dadmohammadi, Y., Nygaard, R., Wood, D., Mokhtari, M., & Salehi, S. (2017). Identification and evaluation of well integrity and causes of failure of well integrity barriers (A review). Journal of Natural Gas Science and Engineering, 45, 511-526.

Koťátková, J., Zatloukal, J., Reiterman, P., & Kolář, K. (2017). Concrete and cement composites used for radioactive waste deposition. Journal of environmental radioactivity, 178, 147-155.

Krakowiak, K. J., Thomas, J. J., James, S., Abuhaikal, M., & Ulm, F.-J. (2018). Development of silica-enriched cement-based materials with improved aging resistance for application in high-temperature environments. Cement and concrete research, 105, 91-110.

Kurashige, M. (1989). A thermoelastic theory of fluid-filled porous materials. International Journal of Solids and Structures, 25(9), 1039-1052.

Massion, C., Radonjic, M., Lu, Y., Bunger, A., & Crandall, D. (2021). Impact of Graphene and the Testing Conditions on the Wellbore Cement Mechanical and Microstructural Properties. Paper presented at the 55th US Rock Mechanics/Geomechanics Symposium. Paper Number: ARMA-2021-2089

Massion, C., Vissa, V. S., Lu, Y., Crandall, D., Bunger, A., & Radonjic, M. (2022). Geomimicry-Inspired Micro-Nano Concrete as Subsurface Hydraulic Barrier Materials: Learning from Shale Rocks as Best Geological Seals. In REWAS 2022: Energy Technologies and CO2 Management (Volume II) (pp. 129-138): Springer.

Meng, M., Frash, L. P., Carey, J. W., Li, W., Welch, N. J., & Zhang, W. (2021). Cement stress and microstructure evolution during curing in semi-rigid high-pressure environments. Cement and concrete research, 149, 106555.

Olson, J., Eustes, A., Fleckenstein, W., Eker, E., Baker, R., & Augustine, C. (2015). Completion Design Considerations for a Horizontal Enhanced Geothermal System. GRC Transactions, 39, 335-344.

Picandet, V., Rangeard, D., Perrot, A., & Lecompte, T. (2011). Permeability measurement of fresh cement paste. Cement and concrete research, 41(3), 330-338.

Qin, J., Pang, X., Cheng, G., Bu, Y., & Liu, H. (2021). Influences of different admixtures on the properties of oil well cement systems at HPHT conditions. Cement and Concrete Composites, 123, 104202.

Roshan, H., Andersen, M., & Acworth, R. (2015). Effect of solid–fluid thermal expansion on thermo-osmotic tests: an experimental and analytical study. Journal of Petroleum Science and Engineering, 126, 222-230.

Samarakoon, M., Ranjith, P., & Wanniarachchi, W. (2022). Properties of well cement following carbonated brine exposure under HTHP conditions: A comparative study of alkali-activated and class G cements. Cement and Concrete Composites, 126, 104342.

Sarout, J., & Detournay, E. (2011). Chemoporoelastic analysis and experimental validation of the pore pressure transmission test for reactive shales. International Journal of Rock Mechanics and Mining Sciences, 48(5), 759-772.

Scholz, M., & Grabowiecki, P. (2007). Review of permeable pavement systems. Building and environment, 42(11), 3830-3836.

Shapiro, A. (2003). Monte Carlo sampling methods. Handbooks in operations research and management science, 10, 353-425.

Skempton, A. (1984). Effective stress in soils, concrete and rocks. Selected papers on soil mechanics, 1032(3), 4-16.

Smith, D. W., & Booker, J. R. (1993). Green's functions for a fully coupled thermoporoelastic material. International Journal for Numerical and Analytical Methods in Geomechanics, 17(3), 139-163.

Snee, J.-E. L., & Zoback, M. D. (2018). State of stress in the Permian Basin, Texas and New Mexico: Implications for induced seismicity. The Leading Edge, 37(2), 127-134.

Song, Z., Liang, F., Lin, C., & Xiang, Y. (2019). Interaction of pore pressures in double-porosity medium: Fluid injection in borehole. Computers and Geotechnics, 107, 142-149.

Stehfest, H. (1970). Algorithm 368: Numerical inversion of Laplace transforms [D5]. Communications of the ACM, 13(1), 47-49.

Tao, Q., & Ghassemi, A. (2010). Poro-thermoelastic borehole stress analysis for determination of the in situ stress and rock strength. Geothermics, 39(3), 250-259.

Trémosa, J., Gonçalvès, J., Matray, J., & Violette, S. (2010). Estimating thermo-osmotic coefficients in clay-rocks: II. In situ experimental approach. Journal of colloid and interface science, 342(1), 175-184.

Valov, A., Golovin, S., Shcherbakov, V., & Kuznetsov, D. (2022). Thermoporoelastic model for the cement sheath failure in a cased and cemented wellbore. Journal of Petroleum Science and Engineering, 210, 109916.

Vrålstad, T., Saasen, A., Fjær, E., Øia, T., Ytrehus, J. D., & Khalifeh, M. (2019). Plug & abandonment of offshore wells: Ensuring long-term well integrity and cost-efficiency. Journal of Petroleum Science and Engineering, 173, 478-491.

Wang, H. F. (2017). Theory of linear poroelasticity with applications to geomechanics and hydrogeology: Princeton University Press.

Wang, Y., & Dusseault, M. B. (2003). A coupled conductive–convective thermo-poroelastic solution and implications for wellbore stability. Journal of Petroleum Science and Engineering, 38(3-4), 187-198.

Weisstein, E. W. (2002). Eigen decomposition. https://mathworld. wolfram. com/.

Xu, S., & Zoback, M. D. (2015). Analysis of stress variations with depth in the Permian Basin Spraberry/Dean/Wolfcamp Shale. Paper presented at the 49th US Rock Mechanics/Geomechanics Symposium. Paper Number: ARMA-2015-189

Zhou, X., & Ghassemi, A. (2009). Finite element analysis of coupled chemo-poro-thermo-mechanical effects around a wellbore in swelling shale. International Journal of Rock Mechanics and Mining Sciences, 46(4), 769-778.

Zoback, M., Barton, C., Brudy, M., Castillo, D., Finkbeiner, T., Grollimund, B., . . . Wiprut, D. (2003). Determination of stress orientation and magnitude in deep wells. International Journal of Rock Mechanics and Mining Sciences, 40(7-8), 1049-1076.